<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.7.5b.07.02.6130" moduleId="e9854a9f43d731fa8b55bb73c4bf412d">
    <author>John De Cristofaro for Adafruit Industries</author>
    <title>Raspberry Pi (Model B)</title>
    <label>Raspberry Pi</label>
    <date>2012-08-04</date>
    <tags>
        <tag>raspberry</tag>
        <tag>pi</tag>
        <tag>adafruit</tag>
        <tag>sbc</tag>
        <tag>arm</tag>
        <tag>model b</tag>
    </tags>
    <properties>
        <property name="family"></property>
        <property name="part number"></property>
    </properties>
    <description>Raspberry Pi Single-board Computer, Model B</description>
    <views>
        <iconView>
            <layers image="icon/Raspberry_Pi__Model_B___00686a34fe2aba68__icon__56f0326763f48a09de38bfea388ae5fa.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/Raspberry_Pi__Model_B___00686a34fe2aba68__breadboard__0e3fd0d0c89756180e5cbda36e8e3197.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/Raspberry_Pi__Model_B___00686a34fe2aba68__schematic__d0e91ee613339a28408d6d0af282a8b6.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/Raspberry_Pi__Model_B___00686a34fe2aba68__pcb__5ec93daa4d94bb6f465d0ace719fc1bc.svg">
                <layer layerId="copper1"/>
                <layer layerId="silkscreen"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector7" type="pad" name="#4">
            <description>GPIO #4</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector7pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector7pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector7pad"/>
                    <p layer="copper0" svgId="connector7pad"/>
                    <p layer="copper1" svgId="connector7pad"/>
                    <p layer="copper0" svgId="connector7pad"/>
                    <p layer="copper0" svgId="connector7pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector15" type="pad" name="#22">
            <description>GPIO #22</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector15pin" terminalId="connector15terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector15pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector15pad"/>
                    <p layer="copper0" svgId="connector15pad"/>
                    <p layer="copper1" svgId="connector15pad"/>
                    <p layer="copper0" svgId="connector15pad"/>
                    <p layer="copper0" svgId="connector15pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector16" type="pad" name="#23">
            <description>GPIO #23</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector16pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector16pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector16pad"/>
                    <p layer="copper0" svgId="connector16pad"/>
                    <p layer="copper1" svgId="connector16pad"/>
                    <p layer="copper0" svgId="connector16pad"/>
                    <p layer="copper0" svgId="connector16pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector8" type="pad" name="TXD">
            <description>Serial TX (output) line</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector8pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector8pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector8pad"/>
                    <p layer="copper0" svgId="connector8pad"/>
                    <p layer="copper1" svgId="connector8pad"/>
                    <p layer="copper0" svgId="connector8pad"/>
                    <p layer="copper0" svgId="connector8pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector18" type="pad" name="#24">
            <description>GPIO #24</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector18pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector18pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector18pad"/>
                    <p layer="copper0" svgId="connector18pad"/>
                    <p layer="copper1" svgId="connector18pad"/>
                    <p layer="copper0" svgId="connector18pad"/>
                    <p layer="copper0" svgId="connector18pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector19" type="pad" name="MOSI">
            <description>SPI MOSI (master out / slave in)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector19pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector19pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector19pad"/>
                    <p layer="copper0" svgId="connector19pad"/>
                    <p layer="copper1" svgId="connector19pad"/>
                    <p layer="copper0" svgId="connector19pad"/>
                    <p layer="copper0" svgId="connector19pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector21" type="pad" name="MISO">
            <description>SPI MISO (master in / slave out)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector21pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector21pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector21pad"/>
                    <p layer="copper0" svgId="connector21pad"/>
                    <p layer="copper1" svgId="connector21pad"/>
                    <p layer="copper0" svgId="connector21pad"/>
                    <p layer="copper0" svgId="connector21pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector22" type="pad" name="#25">
            <description>GPIO #25</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector22pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector22pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector22pad"/>
                    <p layer="copper0" svgId="connector22pad"/>
                    <p layer="copper1" svgId="connector22pad"/>
                    <p layer="copper0" svgId="connector22pad"/>
                    <p layer="copper0" svgId="connector22pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector23" type="pad" name="SCLK">
            <description>SPI clock</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector23pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector23pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector23pad"/>
                    <p layer="copper0" svgId="connector23pad"/>
                    <p layer="copper1" svgId="connector23pad"/>
                    <p layer="copper0" svgId="connector23pad"/>
                    <p layer="copper0" svgId="connector23pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector24" type="pad" name="CS0">
            <description>SPI chip select 0</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector24pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector24pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector24pad"/>
                    <p layer="copper0" svgId="connector24pad"/>
                    <p layer="copper1" svgId="connector24pad"/>
                    <p layer="copper0" svgId="connector24pad"/>
                    <p layer="copper0" svgId="connector24pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector26" type="pad" name="CS1">
            <description>SPI chip select 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector26pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector26pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector26pad"/>
                    <p layer="copper0" svgId="connector26pad"/>
                    <p layer="copper1" svgId="connector26pad"/>
                    <p layer="copper0" svgId="connector26pad"/>
                    <p layer="copper0" svgId="connector26pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" type="pad" name="3V3">
            <description>3.3V power rail (from onboard LDO)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pad"/>
                    <p layer="copper0" svgId="connector1pad"/>
                    <p layer="copper1" svgId="connector1pad"/>
                    <p layer="copper0" svgId="connector1pad"/>
                    <p layer="copper0" svgId="connector1pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector10" type="pad" name="RXD">
            <description>Serial RX (input) line</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector10pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector10pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector10pad"/>
                    <p layer="copper0" svgId="connector10pad"/>
                    <p layer="copper1" svgId="connector10pad"/>
                    <p layer="copper0" svgId="connector10pad"/>
                    <p layer="copper0" svgId="connector10pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector2" type="pad" name="5V">
            <description>5V power rail (from USB)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector2pad"/>
                    <p layer="copper0" svgId="connector2pad"/>
                    <p layer="copper1" svgId="connector2pad"/>
                    <p layer="copper0" svgId="connector2pad"/>
                    <p layer="copper0" svgId="connector2pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector3" type="pad" name="SDA">
            <description>I2C/TWI data</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector3pad"/>
                    <p layer="copper0" svgId="connector3pad"/>
                    <p layer="copper1" svgId="connector3pad"/>
                    <p layer="copper0" svgId="connector3pad"/>
                    <p layer="copper0" svgId="connector3pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector11" type="pad" name="#17">
            <description>GPIO #17</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector11pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector11pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector11pad"/>
                    <p layer="copper0" svgId="connector11pad"/>
                    <p layer="copper1" svgId="connector11pad"/>
                    <p layer="copper0" svgId="connector11pad"/>
                    <p layer="copper0" svgId="connector11pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector12" type="pad" name="#18">
            <description>GPIO #18</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector12pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector12pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector12pad"/>
                    <p layer="copper0" svgId="connector12pad"/>
                    <p layer="copper1" svgId="connector12pad"/>
                    <p layer="copper0" svgId="connector12pad"/>
                    <p layer="copper0" svgId="connector12pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector5" type="pad" name="SCL">
            <description>I2C/TWI clock</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector5pad"/>
                    <p layer="copper0" svgId="connector5pad"/>
                    <p layer="copper1" svgId="connector5pad"/>
                    <p layer="copper0" svgId="connector5pad"/>
                    <p layer="copper0" svgId="connector5pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector13" type="pad" name="#21">
            <description>GPIO #21</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector13pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector13pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector13pad"/>
                    <p layer="copper0" svgId="connector13pad"/>
                    <p layer="copper1" svgId="connector13pad"/>
                    <p layer="copper0" svgId="connector13pad"/>
                    <p layer="copper0" svgId="connector13pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector6" type="pad" name="GND">
            <description>System Ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector6pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector6pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector6pad"/>
                    <p layer="copper0" svgId="connector6pad"/>
                    <p layer="copper1" svgId="connector6pad"/>
                    <p layer="copper0" svgId="connector6pad"/>
                    <p layer="copper0" svgId="connector6pad"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
